tML® - Rack Mount Enclosures 19''/3U black for 17 x modules 5HP

\*\*tML® - tde Modular Link

tML® is a patented, modular cabling system consisting of the three key components module, trunk cable and rack mount enclosure. The system components are 100 percent manufactured, pre-assembled and tested in Germany. They enable plug-and-play installation on site – especially in data centres, but also in industrial environments – within the shortest possible time. Heart of the system are the rear MPO/MTP® and Telco connectors, which can be used to connect at least six or twelve ports at a time. Depending on the module configuration, transfer rates of up to 200G are currently possible with SR4. The fibre optic and TP modules can be used together in a module carrier with a very high port density. The tde offers its tML® cabling system as a proven tML® standard system and in the highly innovative variants tML® Xtended, tML® 24 System and now tML® 32 System for extreme scalability and very easy migration to higher transmission rates such as 40G, 100G, 200G and 400G.

\*\*tML® - Rack Mount Enclosures 3U + Accessories

The Rack Mount Enclosure 19“/3U is for the equip of up to 17 x tML® - modules 5HP with high component density.

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Box | Galvanized steel sheet with grounding screw |
| Frontplate | black |
| Inscription | by means of label strips |
| Equip | up to 17 modules, i.e. up to 102 RJ45-Ports or 2448 fibres with MPO/MTP® technology. The combination of different modules is possible. |
| Strain Relief | by means of cable straps at the means cross beam |
| Measures | 19“, 3U, depth 24cm |
|  | QS-Managementsystem ISO 9001, ISO 14001 and TL 9000 |