FO Splice cassette for up to 24x splices

\*\*FO Components

\*\*FO Splice Accessories

The fiber optic splice cassette takes twelve fusion splices with crimp or heat shrink protectors.
• 3x straight cable entries and 1x angled cable entry
• locking receptacle for crimp or shrink splice holder
• Inter locking system for the cassette cover
• Support for fiber strain relief element
• holes for cartridge hinge
• labeling field
• 2x large fiber cutouts in the cassette bottom
• Stackable
• Telecom approval

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | Splice cassette |
| Dimensions | 155 x 92 x 8 mm |
| Material | Bright ABS, similar RAL 1013 |