FO overlength cassette short

\*\*FO Components

\*\*FO Splice Accessories

The FO overlength cassette has two latching noses for the cassette cover. The cassette bottom has two large fiber cutouts.

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | overlength cassette short |
| Dimensions | 135 x 92 x 18 mm |
| Material | Bright ABS, similar RAL 1013 |