2.5Gbps SFP Module MM LC 550m data range (850nm)

\*\*GBIC-, SFP-, XFP-, XENPAK-Transceiver

The tde Small Form Pluggable Optical Transceiver are easy installed for enterprise and telecom applications. The tde SFP modular line provides a fully compatible, highly reliable and volume accessible supply of quality transceiver products with excellent performance for design-in manufacturing and end-user enterprise applications.

\*\*SFP Modules

\*\*TECHNISCHE\_DATEN

Features
• Operating data rate up to 2.5Gbps
• 850nm VCSEL Laser Transmitter
• 300m with 50/125 μm MMF, 150m on 62.5/125 μm MMF
• Single 3. 3V Power supply and TTL Logic Interface
• Duplex LC Connector Interface
• Hot Pluggable
• Operating Case Temperature Industrial: -40°C~+85°C
• Compliant with MSA SFP Specification
• Digital diagnostic monitor interface Compatible with SFF-8472
Applications
• Gigabit Ethernet Switches and Routers
• Fiber Channel Switch Infrastructure
• XDSL Applications
• Metro Edge Switching

|  |  |  |
| --- | --- | --- |
| Features | Standard | Performance |
| Electrostatic Discharge (ESD) to the Electrical Pins | MIL-STD-883E Method 3015.7 | Class 1(>500 V) Isolation with the case |
| Electromagnetic Interference (EMI) | FCC Part 15 Class B | Compatible with standards |
| Laser Eye Safety | FDA 21CFR 1040.10 and 1040.11 EN60950, EN (IEC) 60825-1,2 | Compatible with Class I laser product. Compatible with T üV standards |
| Component Recognition | UL and CUL | UL file E317337 |
| Green Products | RoHS | RoHS6 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Symbol | Min. | Max. | Unit |
| Storage Temperature | TS | -40 | +85 | °C |
| Supply Voltage | VCC | -0.5 | 3.6 | V |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | Symbol | Min. | Typ. | Max. | Unit |
| Operating Case Temperature | TA  /  A2S2-SX | -40 |  | +85 | °C |
| Power Supply Voltage | VCC | 3.15 | 3.3 | 3.45 | V |
| Total Supply Current | ICC |  |  | 300 | mA |
| Surge Current | ISurge |  |  | +30 | mA |
| Baud Rate |  | 1.063 |  | 2.5 | GBaud |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Parameter | Symbol | Min. | Typ. | Max. | Unit | Notes |
| Transmitter |  |  |  |  |  |  |
| LVPECL Inputs (Differential) | Vin | 400 |  | 2500 | mVp | AC coupled inputs |
| Input Impedance (Differential) | Zin | 85 | 100 | 115 | ohms | Rin > 100 kohms @ DC |
| Tx\_DISABLE Input Voltage - High |  | 2 |  | 3.45 | V |  |
| Tx\_DISABLE Input Voltage - Low |  | 0 |  | 0.8 | V |  |
| Tx\_FAULT Output Voltage - High |  | 2 |  | Vcc+0.3 | V | Io = 400μA; Host Vcc |
| Tx\_FAULT Output Voltage - Low |  | 0 |  | 0.5 | V | Io = -4.0mA |
| Receiver |  |  |  |  |  |  |
| LVPECL Outputs (Differential) | Vout | 400 | 800 | 1200 | mVpp | AC coupled outputs |
| Output Impedance (Differential) | Zout | 85 | 100 | 115 | ohms |  |
| Rx\_LOS Output Voltage - High |  | 2 |  | Vcc+0.3 | V | lo = 400μA; Host Vcc |
| Rx\_LOS Output Voltage - Low |  | 0 |  | 0.8 | V | lo = -4.0mA |
| MOD\_DEF ( 0:2 ) | VoH VoL | 2.5 0 |  | 0.5 | V V | With Serial ID |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Parameter | Symbol | Min. | Typ. | Max. | Unit |
| 50μm Core Diameter MMF -1.063G -2.125G | L L | 500 300 |  | m m |
| 62.5μm Core Diameter MMF -1.063G -2.125G | L L |  | 300 150 |  | m m |
| Data Rate |  |  | 2.5 |  | Gbps |
| Transmitter |  |  |  |  |  |
| Centre Wavelength | λc | 820 | 850 | 860 | nm |
| Spectral Width (RMS) | σ |  |  | 0.85 | nm |
| Average Output Power | P 0ut | -10 |  | -4 | dBm |
| Extinction Ratio | EX | 9 |  |  | dB |
| Rise/Fall Time (20% − 80%) | tr/tf |  |  | 160 | ns |
| Output Optical Eye | ITU-T G.957 Compliant |  |  |  |  |
| Data Input Swing Differential | V IN | 500 |  | 2000 | mV |
| Input Differential Impedance | ZIN | 90 | 100 | 110 | Ω |
| TX Disable - Disable                 - Enable |  | 2.0 0 |  | VCC+0.3 0.8 | V V |
| TX\_Fault - Fault              - Normal |  | 2.0 0 |  | VCC+0.3 0.8 | V V |
| TX\_Disable Assert Time | t\_off |  |  | 10 | us |
| Receiver |  |  |  |  |  |
| Centre Wavelength | λc | 760 |  | 860 | nm |
| Sensitivity | PIN |  |  | -15 | dBm |
| Output Differential Impedance | P IN | 90 | 100 | 110 | Ω |
| Data Output Swing Differential | VOUT | 370 |  | 2000 | mV |
| Rise/Fall Time | Tr/tf |  |  | 2.2 | ns |
| LOS De-Assert | LOSD |  |  | -16 | dBm |
| LOS Assert | LOSA | -30 |  |  | dBm |
| LOS  -High         -Low |  | 2,0 0 |  | VCC+0.3 0.8 | V V |