tBL® - Wall mount enclosure 300x300x85mm lockable, sidewalls removable

\*\*tBL® - tde Basic Link (FO Enclosures)

The FO enclosures of the tBL® - tde Basic Link series are optimized products with a high functionality and an easy handling at the installation. The program includes splice and breakout boxes for 19 inch, wall and DIN rail mounting. These products are characterized by a high port density and an optimal fiber management, so that the permissible bending radii can't be undercut. Moreover, there are no sharp corners or edges, to avoid damage to the pigtails and buffer tubes. The front plates are removable. There are versions for E2000, FC, PC, LC, MPO / MTP, MTRJ, MU, SC, and ST. These products can be obtained with or without equipment. In addition, there are also special versions with IP66 for outdoor and offshore applications.

\*\*Wall Mount Enclosures

The compact housing can be used as splice distributor of the fiber optic trunk cable or used as an office distribution.

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Material | Steel sheet 1.5 mm |
| Color | 7035 |
| Dimensions | 300 x 300 x 85 mm (H x W x D) |
| Pre-mounted | 1x small housing |
|  | 2x side panel removed without tools, sheet steel 1 mm, RAL 7035 |
|  | 1x door lockable, sheet steel 1 mm, RAL 7035 |
|  | 1x cassettes splice holder quadruple |
|  | 1x set wall mounting material |
| Norms | DIN 50173 |
| Protection class | IP 20 |
|  | QS-Managementsystem ISO 9001, ISO 14001 and TL 9000 |