tBL® - set of cable entry plates M20/M16 for wall mount enclosure

\*\*tBL® - tde Basic Link (FO Enclosures)

The FO enclosures of the tBL® - tde Basic Link series are optimized products with a high functionality and an easy handling at the installation. The program includes splice and breakout boxes for 19 inch, wall and DIN rail mounting. These products are characterized by a high port density and an optimal fiber management, so that the permissible bending radii can't be undercut. Moreover, there are no sharp corners or edges, to avoid damage to the pigtails and buffer tubes. The front plates are removable. There are versions for E2000, FC, PC, LC, MPO / MTP, MTRJ, MU, SC, and ST. These products can be obtained with or without equipment. In addition, there are also special versions with IP66 for outdoor and offshore applications.

\*\*Wall Mount Enclosures

The cable entry plates are used to receive metric cable glands in the wall mount enclosure.

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | 2x Cable entry plate M20/M16 |
| Configuration | Attachment of cable entrys M20/M16 |