MPO/MTP® Adapter with Flange, Type A, green (APC)

\*\*FO Components

\*\*FO Adapters

• One piece adapter design maximizes coupling strength while minimizing debris generation
• All adapters compatible with MTP Elite® brand connectors and standard grade MTP® brand connectors
• Available in black, magenta, aqua, beige, green, blue and gray
• Supplied with either one or two thermoplastic non-debris generating dust plugs
• Compatible with all US Conec MPO/MTP® brand connectors in fiber counts ranging 12 and 24
• Optimal coarse alignment to minimize pin to ferrule debris generation

Applications

• Array trunk cabling
• Array fiber to single fiber cassettes
• High fiber density card edge access
• Optical switching interframe connections
• Meets IEC Standard 61754-7
• Meets TIA/EIA 604-5 Type MPO
• Structured cabling per TIA-568-C
• Parallel Optics

• Optical Internetworking Forum (OIF) Compliant
• Infiniband Compliant
• 10G Fiber Channel Compliant
• 40G and 100G IEEE 802.3
• SNAP 12
• POP 4
• QSFP

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | MPO/MTP® |
| Application | Singlemode OS2 APC |
| Design | with Flange |
| Connector style | MPO/MTP®  |
| Key Orientation | Type A, Key up/down |
| Color | Green |
| Material | Plastic |
| Sleeve | -- |
| Shutter | -- |
| Standards | IEC 61754-7 TIA 604-5 |
| Manufacturer | US Conec |