tBL® - FO breakout panel 19" 1U 12 LC Duplex Adapter, beige

\*\*tBL® - tde Basic Link (FO Enclosures)

The FO enclosures of the tBL® - tde Basic Link series are optimized products with a high functionality and an easy handling at the installation. The program includes splice and breakout boxes for 19 inch, wall and DIN rail mounting. These products are characterized by a high port density and an optimal fiber management, so that the permissible bending radii can't be undercut. Moreover, there are no sharp corners or edges, to avoid damage to the pigtails and buffer tubes. The front plates are removable. There are versions for E2000, FC, PC, LC, MPO / MTP, MTRJ, MU, SC, and ST. These products can be obtained with or without equipment. In addition, there are also special versions with IP66 for outdoor and offshore applications.

\*\*FO Splice Boxes

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Alternative pre-mounted | TBL-PF24-xxLCD-BG (see below) |
| xx | (01 - 24) quantity of adapters |

\*\*\*FO Splice Boxes

|  |  |
| --- | --- |
| Type | Breakout panel with cable catch |
| Material | Sheet steel |
| Color | RAL 7035 |
| Dimensions | 19'' 1U 240mm depth |
| Labeling | 1 - 24 (silk screen) |
| Configuration | Attachment up to 24x SC Simplex, LC Duplex, E2000 Simplex or MPO adapter |

|  |  |
| --- | --- |
| Type | FO Blind stopper |
| Application | For covering of unused adapter slots |

|  |  |
| --- | --- |
| Type | Mounting set M5 |
|  | Set of 4 (cage nuts and screws) |