TN-CWDM-SFP-1xx0-16 - Cisco Compatible CWDM SFP Modules, 1000Base-LX/ZX Fiber Channel (LC) [160 km/99.4 mi.]

\*\*Lantronix / Transition Networks

\*\*Direct Attach Cables / Active Optical Cables

A simple to install, cost-effective and interoperable solution
Often used for data center short-reach interconnects, Direct Attach, Active Copper and Active Optical Cables are an indispensable part of any network.
Terminated with transceiver-style connectors, they are designed to be used in the same ports as a typical SFP+ or QSFP transceiver, with no need for adapters or converters. Our DAC and AOC cables offer compatibility with a huge range of vendors, enabling the connectivity you need within the Top of Rack and End of Row environments.
• 10G, 25G, 40G & 100G product solutions
• Seamless interoperability with network equipment
• Multi-code options enabling different OEM vendors at each end of the cable
• 4x breakout cables, 40G QSFP+ to 4x 10G SFP and 100G QSFP28 to 4x 25G SFP28
• Fast Delivery, Custom solutions
• Compatible with Over 90 Systems
• Savings of up to 70%

\*\*Transition Networks - Optical Devices

1000Base-LX/ZX Fiber Channel single mode (LC) with DMI 1590nm [160 km/99.4 mi.] Link Budget: 36.0 dB
\*\*Product Description
1000Base-LX/ZX Fiber Channel single mode (LC) with DMI [160 km/99.4 mi.] Link Budget: 36.0 dB
\*\*Features
• Coarse Wavelength Division Multiplexing (CWDM) ITU Grid Compliant Wavelength
• Hot-Pluggable SFP Optical Transceiver With Duplex LC Connector
• Digital Diagnostic Function (DMI)
• Class 1 Laser International Safety Standard IEC-60825 Compliant
• Compatible with SFP Multi-Sourcing Agreement (MSA)
• Single +3.3V Power Supply
• RoHS Compliant
• Compliant with IEEE 802.3z 1000Base-LX/ZX
• Compliant with Fiber Channel 1x SM-LC-L FC-PI
• Compliant with IEEE 802.3z 1000Base-LX/ZX
• Compliant with Fiber Channel
• 1x SM-LC-L FC-PI
Show product on manufacturers website: https://www.lantronix.com/products/

\*\*TECHNISCHE\_DATEN

\*\*Specifications