10GBase-BX, SFP+ with DMI 1270nm TX/1330nm RX single fiber single mode (LC) [20 km/12.4 mi.] Link Budget: 12.1 dB

\*\*Lantronix / Transition Networks

\*\*Direct Attach Cables / Active Optical Cables

A simple to install, cost-effective and interoperable solution
Often used for data center short-reach interconnects, Direct Attach, Active Copper and Active Optical Cables are an indispensable part of any network.
Terminated with transceiver-style connectors, they are designed to be used in the same ports as a typical SFP+ or QSFP transceiver, with no need for adapters or converters. Our DAC and AOC cables offer compatibility with a huge range of vendors, enabling the connectivity you need within the Top of Rack and End of Row environments.
• 10G, 25G, 40G & 100G product solutions
• Seamless interoperability with network equipment
• Multi-code options enabling different OEM vendors at each end of the cable
• 4x breakout cables, 40G QSFP+ to 4x 10G SFP and 100G QSFP28 to 4x 25G SFP28
• Fast Delivery, Custom solutions
• Compatible with Over 90 Systems
• Savings of up to 70%

\*\*Optics

Applications include: 10G Ethernet Switches and Routers and Metro Edge Switching.
\*\*\*Features
• SFP+ Optical Transceiver with LC connector
• 10G Small Form-Factor Pluggable (SFP+) MSA Compliant
• Compliant with 10GBase-BX
• SFF-8472 Digital Diagnostic Function (DMI)
• Maximum Link Length of 80 km
• Single +3.3V Power Supply
• RoHS Compliant

\*\*TECHNISCHE\_DATEN

\*\*\*Standards
• IEEE 802.3z
• IEEE 802.3
• IEEE 802.3ae
\*\*\*Output Wavelength
• -5.5nm <λc < +7.5nm
\*\*\*Dimensions
• Width: 0.52” [13 mm]
• Depth: 2.18” [55 mm]
• Height: 0.33” [8 mm]
\*\*\*Power Input
• 3.3V
\*\*\*Environment
• Operating: 0°C to 70°C
• Storage: -40°C to 85°C
\*\*\*Certifications
• IEC-60825, FDA 21, CFR 1040.10 and 1040.11
\*\*\*Warranty
• Lifetime