PS, 90W, 48V, LEVEL 6 ADAPTER, W/KYCON KPPX-4P CONN, CUSTOM, AR P/S

\*\*Lantronix / Transition Networks

\*\*Direct Attach Cables / Active Optical Cables

A simple to install, cost-effective and interoperable solution

Often used for data center short-reach interconnects, Direct Attach, Active Copper and Active Optical Cables are an indispensable part of any network.

Terminated with transceiver-style connectors, they are designed to be used in the same ports as a typical SFP+ or QSFP transceiver, with no need for adapters or converters. Our DAC and AOC cables offer compatibility with a huge range of vendors, enabling the connectivity you need within the Top of Rack and End of Row environments.

• 10G, 25G, 40G & 100G product solutions
• Seamless interoperability with network equipment
• Multi-code options enabling different OEM vendors at each end of the cable
• 4x breakout cables, 40G QSFP+ to 4x 10G SFP and 100G QSFP28 to 4x 25G SFP28
• Fast Delivery, Custom solutions
• Compatible with Over 90 Systems
• Savings of up to 70%

\*\*Media Converters

90 ~ 264 VAC; 127 ~ 370 VDC

\*\*Features

• Universal AC input/full range
• 3 pole AC inlet IEC320-C14
• Built-in active power factor controller function
• Industrial (-30°C to +70°C) operating temperature
• No load power consumption â¤0.15 Watts
• Energy efficiency Level VI
• Compliant with EIASA 2007/DoE, NRCan, AU/NZ MEPS, EU ErP and CoC Version 5
• Class 1 power (with earth pin)
• Short circuit/overload/over voltage/over temperature protection
• Fully enclosed 94V-0 flame retardant plastic case
• LED power on indicator

Show product on manufacturers website: https://www.lantronix.com/products/

\*\*TECHNISCHE\_DATEN