Mini Media Converter 1000Base-T RJ-45 to 1000Base-SX MM LC W/ -JP Power

\*\*Lantronix / Transition Networks

\*\*Direct Attach Cables / Active Optical Cables

A simple to install, cost-effective and interoperable solution

Often used for data center short-reach interconnects, Direct Attach, Active Copper and Active Optical Cables are an indispensable part of any network.

Terminated with transceiver-style connectors, they are designed to be used in the same ports as a typical SFP+ or QSFP transceiver, with no need for adapters or converters. Our DAC and AOC cables offer compatibility with a huge range of vendors, enabling the connectivity you need within the Top of Rack and End of Row environments.

• 10G, 25G, 40G & 100G product solutions
• Seamless interoperability with network equipment
• Multi-code options enabling different OEM vendors at each end of the cable
• 4x breakout cables, 40G QSFP+ to 4x 10G SFP and 100G QSFP28 to 4x 25G SFP28
• Fast Delivery, Custom solutions
• Compatible with Over 90 Systems
• Savings of up to 70%

\*\*Converters and Device Servers

\*\*TECHNISCHE\_DATEN