E2000™ Simplex Adapter ceramic with flange, magenta/magenta, class M

\*\*E2000™ Adapter

Wherever high-end solutions are required, R&M relies on its E-2000™ family of connectors. R&M is one of only three manufacturers worldwide to manufacture this standardized high-performance connector (manufactured under license from Diamond SA, Losone). The optimum transmission properties of this push-pull connector are based on high-precision ceramic ferrules, adapted interfaces for improved insertion and return losses, and APC 8° ferrules for high-return loss requirements. High quality is guaranteed throughout. 100% of the assemblies are tested directly in the process. The self-closing screen not only provides protection against dust and damage, but also protects your maintenance personnel from high-energy laser light. R&M connectors comply with all the relevant European and international standards (CECC 86 275-801, CECC 86 275-802 and IEC 61 754-15).
• Injection-molded PBT housing, UL 94 V-0 (flammability index)
• Integrated, spring-loaded shutters for dust and scratching
  protection
• Long guiding section of connector body
• Split ceramic sleeve/phosphor bronze sleeve
• 1000 mating cycles (zirconia ceramic alignment sleeve)
• 500 mating cycles (phosphor bronze alignment sleeve)

\*\*FO Adapters

Scope of supply
• Adapter E2000™
• 2 Philips head screws M2 x 8, blue galvanized
• 2 mounted hexagonal nuts M2, blue galvanized

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Standardisation: | acc. to IEC61754-15, DIN EN 186270 |
| Connector class: | coupling Adapter |
| Number of connectors (A): | 1 |
| Connector type (A): | E2000™ |
| Protection class (IP) connector (A): | 20 |
| Polishing connector (A): | PC |
| Attenuation grade IL - connector (A): | M |
| Delta insertion loss: | ≤ 0.2 dB, testing method acc. to IEC 61300-3-4 |
| Mating cycles: | min. 1000 |
| Pull-out force: | min. 70 N |
| Connector color (A): | magenta |
| Lever- frame-coding connector (A): | color |
| Frame color connector (A): | magenta |
| Sleeve material: | ceramic |
| Adapter fastening method: | end cap |
| Fiber type: | Multimode (MM) |
| Dimensions: | 74.7 / 42 x 22 x 9.35 mm |
| Material: | plastic: PBT, fiber-glass reinforced (halogen-free) |
| Manufacturer: | R&M |