FC APC Round Adapter, "D" STYLE, Zirconia Straight Split

\*\*FO Components

\*\*FO Adapters

FC Round Adapters come with a D Flange (ø8.85 x 7.95mm), and feature nickel plated brass housing for corrosion resistance.

• Compact design
• NTT-FC compatibility
• High precision alignment
• Low insertion and return loss and back reflection
• Corrosion resistant body

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | FC Simplex |
| Applikation | Singlemode/Multimode |
| Design | Round "D" Style |
| Built form | FC Round |
| Material | Metal |
| Sleeve | Zirconia Straight Split |
| Shutter | -- |
| Manufacturer | tde |