FO cassette cover for overlength cassette short

\*\*FO Components

\*\*FO Splice Accessories

The cover is only suitable for the short FO overlength cassette. It comprises two latching noses, which allow a secure fixing of the cassette.

\*\*TECHNISCHE\_DATEN

|  |  |
| --- | --- |
| Type | Cassette cover short |
| Dimensions | 115 x 92 x 2 mm |
| Material | Bright ABS, similar RAL 1013 |